# SUBBASE GRANULAR MATERIAL TYPE A

Eff. 07-01-2020

Where small quantities of lime modification are shown in the plans, subbase, granular material, Type A may be substituted and constructed according to the applicable portions of Section 311.

The depth of the subbase granular material shall be the same as the proposed depth of the lime modification. This work shall be paid for at the contract unit price per square yard for PROCESSING LIME MODIFIED SOILS of the depth specified.