# GUARD POSTS

Eff. 03-05-1997 Rev. 01-01-2014

This work shall consist of furnishing and setting guard posts according to Section 634 of the Standard Specifications except as follows:

1. The cross section of the posts shall be nominal 4 inches by 4 inches (100 mm by 100 mm.)
2. The tops of the posts shall not be rounded, but shall be sloped at 30 degrees to the horizontal.
3. The length of the posts shall be 5 feet (1.5 m).
4. The embedment of the posts shall be 33 inches (0.84 m.)

* For closure of median ditch checks, the nominal spacing of the posts shall be 5 feet (1.5 m.)