# 5F

# BRIDGE DECK LATEX OR MICROSILICA CONCRETE OVERLAY, CUT OFF DATE

(Effective January 12, 2010)

Placement of concrete for latex or microsilica overlays shall be between April 1 and October 31 unless approved, in writing, by the Engineer.

DESIGNER NOTE:

This work must also include a completion date no later than November 15 or a traffic control special provision requiring the Contractor to schedule his operations so that all traffic lanes are open from December 1 to March 1. This is per a request from Project Implementation to eliminate lane closures/reductions over winter months.