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	This Check Sheet contains a listing of frequently used RECURRING SPECIAL PROVISIONS.

CHECK
SHEET #	PAGE

  1	   91	Additional State Requirements for Federal-aid Construction Contracts
			(Eff 2-1-69) (Rev 1-1-17)  (Include if project has Federal Funds.)

  2	   94	SUBLETTING OF CONTRACTS (Federal Aid Contracts) (Eff 1-1-88)
			(Rev 1-1-14)  (Include if project has Federal Funds.)

  3	   95	EEO (Eff 7-21-78)(Rev 11-18-80)
			(Include on all projects.)

  4	 105		Specific EEO Responsibilities Non-Federal-aid
		Contracts (Eff 3-20-69) (Rev 1-1-94) (Include if project has Straight State Funds.)

  5	 110	Required Provisions - State Contracts (Eff 4-1-65) (Rev 1-1-17)
		(Include if project has Straight State Funds.)

  6	 116	ASBESTOS BEARING PAD REMOVAL (Eff 11-1-03)
			(Include when using the pay items ASBESTOS BEARING PAD REMOVAL)

  7     	 117	ASBESTOS WATERPROOFING MEMBRANE AND ASBESTOS HOT-MIX ASPHALT SURFACE REMOVAL (Eff 6-1-89) (Rev 1-1-09)
			(Include if asbestos is in waterproofing membrane system, experimental on bridges 1968-1975.)

  8	 118	TEMPORARY STREAM CROSSINGS, AND IN-STREAM WORK PADS
			(Eff 1-2-92)(Rev 1-1-98)
			(Use on all bridge projects and multi-cell box culverts in streams with running
		 	water.)

  9	 119	CONSTRUCTION LAYOUT STAKES (Eff 5-1-93)(Rev 1-1-22)
			(Ask Construction field engineer on the Final Field Check if he wants it.)

10	 122	USE OF GEOTEXTILE FABRIC FOR RAILROAD CROSSING
			(Eff 1-1-95)(Rev 1-1-22)

11	 124	SUBSEALING OF CONCRETE PAVEMENTS  (Eff 11-1-84)(Rev 1-1-07)
			(Use with pay items Dry Grout Solids and Holes Drilled.  When using this
			include District Standard 44.4 in the plans.)



12	 128	HOT-MIX ASPHALT SURFACE CORRECTION (Eff 11-1-87) (Rev 1-1-09)
			(Use on projects which do not call for resurfacing 
			When using this include District Standard 43.4 in the plans.)

13	 130 	PAVEMENT & SHOULDER RESURFACING (Eff 2-1-00) (Rev 1-1-09)
			(This special provision shall be included in all resurfacing projects on all four-lane
interstates and other freeways, all four lane expressways, other four lane highways where the ADT exceeds 25,000 or peak one-way VPH exceeds 1700, and two lane highways where the ADT exceeds 10,000 or peak one-way VPH exceeds 800, and where significant traffic delays are expected.)

14	 131	PATCHING WITH HOT-MIX OVERLAY REMOVAL (Eff 10-1-95) (Rev 1-1-18)
			(Use for patching with bituminous overlay.)

15		 133	POLYMER CONCRETE (Eff 8-1-95) (Rev 4-1-16)
				(Include in projects using the pay item POLYMER CONCRETE)
				(Add District Standard 29.4 to the plans.)

16	 135	RESERVED

17	 136	BICYCLE RACKS (Eff 4-1-94)(Rev 1-1-19)
			(Include in all projects using bicycle racks.)

18	 138	TEMPORARY PORTABLE BRIDGE TRAFFIC SIGNALS (EFF 8-1-03) 
			(Rev 1-1-07)
			(Include in all staged bridge contracts that require temporary bridge traffic signals.  This gives the contractor the option of post mounted signals or portable signals.)

19	 140	NIGHT TIME INSPECTION OF ROADWAY LIGHTING (Eff 5-1-96)
			(Include on all projects containing roadway lighting.)

20		 141	ENGLISH SUBSTITUTION OF METRIC BOLTS (Eff 7-1-96) (Rev 1-1-14)
			(Include in all metric projects containing metric bolts.)

21	 142	CALCIUM CHLORIDE ACCELERATOR FOR PORTLAND CEMENT CONCRETE
			(Eff 1-1-01) (Rev 1-1-13)
			(Do not use this in District 2.)

22	 143	QC OF CONCRETE MIXTURES AT THE PLANT (Eff 8-1-00) (Rev 1-1-22)
		(Not used in District 2)

23	 151	QC/QA OF CONCRETE MIXTURES (Eff 4-1-92) (Rev 1-1-22)
(Include in all contracts with cast-in-place concrete)

24	 167	RESERVED

25	 168	RESERVED

26	 169	TEMPORARY RAISED PAVEMENT MARKERS (EFF 1-1-09) (REV 1-1-14)
(Include in preventative maintenance projects requiring cape seals or bituminous surface.)

27	 170	RESTORING BRIDGE APPROACH PAVEMENTS USING HIGH-DENSITY FOAM
(EFF 1-1-09) (REV 1-1-12)
(Include in projects using high-density expanding polyurethane foam for restoring the elevation of settled bridge approach pavements.)

28	 173	PORTLAND CEMENT CONCRETE INLAY OR OVERLAY (EFF 11-1-08) 
		(REV 1-1-22)
(This is an alternative rehabilitation strategy to HMA overlays on pavement or intersections that have experienced excess rutting.  Use of this special provision shall be according to BDE Manual Chapter 53-4.08.  Discuss this with your Project Engineer before using it.)

29	 177	PORTLAND CEMENT CONCRETE PARTIAL DEPTH HOT-MIX ASPHALT PATCHING (EFF 4-1-14) (REV 1-1-18)
(Use on resurfacing projects with bare concrete that needs repair, but does not warrant full-depth patching.)

[bookmark: _Hlk52274789]30	 180	LONGITUDINAL JOINT AND CRACK PATCHING
(EFF 4-1-14) (REV 1-1-20)
(Do not use in District 2)

31	 182	CONCRETE MIX DESIGN DEPARTMENT PROVIDED
(EFF 1-1-12) (REV 4-1-16)
(Include in all contracts with cast-in-place concrete.)

32	 183	STATION NUMBERS IN PAVEMENTS OR OVERLAYS
		(EFF 1-1-22)
		(Do not use in District 2)
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