

**Memorandum**

To: Studies and Plans Squads PPM 80-01

From: C. D. Latham Revised By: Scott Neihart

Subject: Conduit-Highway Lighting

Date: September 9, 1985 Revised Date: April 1, 2016

**PLAN PREPARATION MEMORANDUM 80-01**

On projects which have highway lighting included as part of the contract, quantities should be included in the plans for UNDERGROUND CONDUIT, PVC, 2” DIAMETER, for placement under Portland Cement Concrete Driveway Pavements where wiring is to be installed.

The conduit should be a minimum of 2 feet deep and extend a minimum of 2 feet beyond the edges of the driveway

A note should be included making the Contractor aware that when a driveway is built half at a time, the conduit will have to be placed half at a time.

80-01.doc