**7AJ**

**CONTROL OF WORK – SMART WORK ZONE**

(Effective March 30, 2023)

The contractor must possess enough equipment to provide the following:

* One Smart Traffic Monitoring (STM) systems and Five (5) Smart Traffic Monitoring devices (STMDs) per direction, described in the SMART TRAFFIC MONITORING SYSTEM special provision.
* Two Real-time Traffic Control (RTTC) Signing units per direction. A unit (two signs, four flashers plus equipment) is described in the SMART TRAFFIC MONITORING SYSTEM special provision and shown in the applicable plan detail.
* Seven Portable Changeable Message Signs (PCMS) per direction, described in the CHANGEABLE MESSAGE SIGN, SPECIAL provision and shown in the applicable plan detail.
* One additional portable changeable message sign (PCMS), described in the changeable message sign, special provision will be required to be positioned \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_to provide construction zone information and, if necessary, details to utilize an alternate route.
* Additional control hardware and devices per direction as described in the SMART TRAFFIC MONITORING SYSTEM special provision.

Designer Note: To be used with D3 SP for Smart Traffic Monitoring System, and plan detail for Smart Work Zone. Modify as needed to match project criteria.