# PORTLAND CEMENT CONCRETE BASE COURSE

Eff. 07-01-2020

The shaded areas of PCC base course constructed adjacent to combination concrete curb and gutter as shown in the plans shall be poured monolithic with the combination concrete curb and gutter.

This work will be measured and included in the contract unit price per square yard for PORTLAND CEMENT CONCRETE BASE COURSE of the thickness specified in the plans.