# WATER SERVICE LINE

Eff. 09-11-1990 Rev. 01-01-2014

Water service line shall meet the specifications for seamless copper water tube, ASTM designation B 88 Type K. The pipe shall be laid sufficiently waving and placed in such a manner as to prevent rupture or breakage from settling of the ground.

The water service line shall be used as an extension for an existing water service pipe. This extension shall be accomplished by the use of adapters or compression fittings as required.

Any excavation made in the subgrade or within 2 feet (600 mm) of the proposed pavement shall be backfilled with Trench Backfill. All other trenches shall be backfilled in the manner specified for Storm Sewers.

This work shall be paid for in accordance with Section 562 of the Standard Specifications.