Regional Engineers

 Jack A. Elston

 Special Provision for Concrete Barrier

 September 27, 2024

This special provision was developed by the Bureau of Design and Environment to update the maximum variation allowed in Concrete Barrier, Double Face before Concrete Barrier, Variable Cross-Section is used.

This special provision should be inserted into contracts with CONCRETE BARRIER.

The districts should include the BDE Check Sheet marked with the applicable special provisions for the January 17, 2025 and subsequent lettings. The Project Coordination and Implementation Section will include a copy in the contract.

80461m

# CONCRETE BARRIER (bde)

Effective: January 1, 2025

Revise the second paragraph of Article 637.12 of the Standard Specifications to read:

“ When a double face concrete barrier with a variable cross-section is required, and the variation exceeds 1/2 in. (13 mm), the barrier will be paid for at the contract unit price per foot (meter) for CONCRETE BARRIER, VARIABLE CROSS-SECTION, of the height specified.”

80461