INDEX

FOR

Supplemental SPECIFICATIONS

AND RECURRING SPECIAL PROVISIONS

Adopted January 1, 2026

This index contains a listing of SUPPLEMENTAL SPECIFICATIONS, frequently used RECURRING SPECIAL PROVISIONS, and LOCAL ROADS AND STREETS RECURRING SPECIAL PROVISIONS.

ERRATA Standard Specifications for Road and Bridge Construction

(Adopted 1-1-22) (Revised 1-1-26)

SUPPLEMENTAL SPECIFICATIONS

|  |  |  |  |
| --- | --- | --- | --- |
| Std. Spec. Sec. | | Page No. | |
| 109 | Measurement and Payment | | 1 |
| 202 | Earth and Rock Excavation | | 2 |
| 204 | Borrow and Furnished Excavation | | 3 |
| 207 | Porous Granular Embankment | | 4 |
| 211 | Topsoil and Compost | | 5 |
| 214 | Grading and Shaping Ditches | | 6 |
| 406 | Hot-Mix Asphalt Binder and Surface Course | | 7 |
| 407 | Hot-Mix Asphalt Pavement (Full-Depth) | | 9 |
| 420 | Portland Cement Concrete Pavement | | 10 |
| 502 | Excavation for Structures | | 11 |
| 504 | Precast Concrete Structures | | 12 |
| 509 | Metal Railings | | 13 |
| 522 | Retaining Walls | | 14 |
| 540 | Box Culverts | | 15 |
| 542 | Pipe Culverts | | 35 |
| 550 | Storm Sewers | | 44 |
| 586 | Granular Backfill for Structures | | 51 |
| 601 | Pipe Drains, Pipe Underdrains, and French Drains | | 52 |
| 630 | Steel Plate Beam Guardrail | | 53 |
| 632 | Guardrail and Cable Road Guard Removal | | 54 |
| 644 | High Tension Cable Median Barrier | | 55 |
| 665 | Woven Wire Fence | | 56 |
| 701 | Work Zone Traffic Control and Protection | | 57 |
| 781 | Raised Reflective Pavement Markers | | 59 |
| 782 | Reflectors | | 60 |
| 801 | Electrical Requirements | | 62 |
| 821 | Roadway Luminaires | | 65 |
| 1003 | Fine Aggregates | | 66 |
| 1004 | Coarse Aggregates | | 67 |
| 1010 | Finely Divided Minerals | | 69 |
| 1020 | Portland Cement Concrete ……… | | 70 |
| 1030 | Hot-Mix Asphalt | | 73 |
| 1040 | Drain Pipe, Tile, and Wall Drain | | 74 |
| 1042 | Precast Concrete Products | | 75 |
| 1061 | Waterproofing Membrane System | | 76 |
| 1067 | Luminaire ……… | | 77 |
| 1097 | Reflectors | | 84 |
| 1102 | Hot-Mix Asphalt Equipment | | 85 |
|  |  | |  |

RECURRING SPECIAL PROVISIONS

The following RECURRING SPECIAL PROVISIONS indicated by an “X” are applicable to this contract and are included by reference:

CHECK SHEET # PAGE NO.

|  |  |  |  |
| --- | --- | --- | --- |
| 1 |  | Additional State Requirements for Federal-Aid Construction Contracts | 87 |
| 2 |  | Subletting of Contracts (Federal-Aid Contracts) | 90 |
| 3 |  | EEO | 91 |
| 4 |  | Specific EEO Responsibilities Nonfederal-Aid Contracts | 101 |
| 5 |  | Required Provisions - State Contracts | 106 |
| 6 |  | Asbestos Bearing Pad Removal | 112 |
| 7 |  | Asbestos Waterproofing Membrane and Asbestos Hot-Mix Asphalt Surface Removal | 113 |
| 8 |  | Temporary Stream Crossings and In-Stream Work Pads | 114 |
| 9 |  | Construction Layout Stakes | 115 |
| 10 |  | Use of Geotextile Fabric for Railroad Crossing | 118 |
| 11 |  | Subsealing of Concrete Pavements | 120 |
| 12 |  | Hot-Mix Asphalt Surface Correction | 124 |
| 13 |  | Pavement and Shoulder Resurfacing | 126 |
| 14 |  | Patching with Hot-Mix Asphalt Overlay Removal | 127 |
| 15 |  | Polymer Concrete | 129 |
| 16 |  | Reserved | 131 |
| 17 |  | Bicycle Racks | 132 |
| 18 |  | Temporary Portable Bridge Traffic Signals | 134 |
| 19 |  | Nighttime Inspection of Roadway Lighting | 136 |
| 20 |  | English Substitution of Metric Bolts | 137 |
| 21 |  | Calcium Chloride Accelerator for Portland Cement Concrete | 138 |
| 22 |  | Quality Control of Concrete Mixtures at the Plant | 139 |
| 23 |  | Quality Control/Quality Assurance of Concrete Mixtures | 147 |
| 24 |  | Reserved | 163 |
| 25 |  | Reserved | 164 |
| 26 |  | Temporary Raised Pavement Markers | 165 |
| 27 |  | Restoring Bridge Approach Pavements Using High-Density Foam | 166 |
| 28 |  | Portland Cement Concrete Inlay or Overlay | 169 |
| 29 |  | Portland Cement Concrete Partial Depth Hot-Mix Asphalt Patching | 173 |
| 30 |  | Longitudinal Joint and Crack Patching | 176 |
| 31 |  | Concrete Mix Design – Department Provided | 178 |
| 32 |  | Station Numbers in Pavements or Overlays | 179 |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |