# 4Y

# timeframe for placement of hma after hma surface removal

(Effective May 28, 2025)

Construction shall be scheduled so that all traffic lane areas of Hot-Mix Asphalt surface removal, except for those to be covered with incidental Hot-Mix Asphalt Surfacing, shall be covered with the first lift of new Hot-Mix Asphalt within 24 hours.  This does not apply to driveways and other areas that will be covered with Incidental Hot-Mix Asphalt Surfacing.

This work will not be paid for separately but shall be included in the cost of the HMA surface removal and resurfacing pay items.

Designer Notes:

* This special provision is intended to limit the amount of time a milled surface is exposed to traffic.  Using this special provision will help to minimize the risk of the roadway falling apart after milling.
* Use when requested by materials or construction and pavement cores or recent experience at the project site indicates this procedure is warranted.
* Include District Special Provision 4T: Drainage Mitigation on Milling and Resurfacing Projects when using this special provision.