**6J**

**REFLECTORS FOR DELINEATORS**

(Effective February 20, 2025)

Description. This work includes installing red reflectors on the back side of delineator posts on interstate exit ramps as indicated on Highway Standard 635001, plan details and schedules.

Replace the table in Article 1097.03 with the following:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Divergence Angle | Entrance Angle | Intensity  Candle Power Per Foot Candle | | |
| Degrees | Degrees | Crystal | Amber | Red |
| 0.2º | 0º | 120.0 | 72.0 | 36.0 |
| 0.2º | +20º | 70.0 | 42.0 | 21.0 |

Method of Measurement. Reflectors will not be measured for payment.

Basis of Payment. This work will be paid for at the contract unit price per each for DELINEATORS.