

**Memorandum**

To: Studies and Plans Squads PPM 60-04

From: C. D. Latham Revised by: Scott Neihart

Subject: Inlet Location Near Entrances

Date: December 19, 1983 Revision Date: April 1, 2016

**PLAN PREPARATION MEMORANDUM 60-04**

In urban sections with curb and gutter, the designer should consider placing an inlet immediately upgrade from entrances. This is especially important where the entrance has a negative grade away from the pavement. The placement of these inlets should be considered in the overall inlet spacing throughout the curb & gutter limits.

60-04.doc