**10A**

# QUALITY CONTROL LABORATORY FOR CONCRETE MIXTURES

Revise Article 1020.16(c)(2) of the Special Provision for Quality Control/Quality Assurance of Concrete Mixtures (BDE) to read:

“(2) Required Plant Tests. Sampling and testing shall be performed at the plant to control production of a mixture. The required minimum Contractor plant sampling and testing is indicated in Article 1020.16(g) Schedule A.”

Add to the end of the second paragraph of Article 1020.16(f)(1) of the Special Provision for Quality Control/Quality Assurance of Concrete Mixtures (BDE):

“Reporting of above documents shall be done using the Department’s electronic reporting system, QC/QA Excel Package.”

Designer Notes:

To be inserted in projects with large quantities of concrete when requested by the Bureau of Materials.

The QC/QA of Concrete Mixtures Special Provision (BDE) must be inserted with this special provision.