**4G**

# VIBRATORY ROLLER RESTRICTION

(Effective: November 26, 2013)

The use of vibratory rollers in dynamic mode shall not be allowed on bridge decks and in urban areas that may include aging infrastructure under the roadway. These locations will be determined in the field by the Engineer.

The restriction of dynamic vibratory rollers in these areas shall not waive density requirements.

**Designer Note:**

Place into all HMA contracts (except PFP) where resurfacing locations include bridge decks and urban areas that may include aging infrastructure under the roadway where vibrations could cause damage.