# SEEDING, CLASS 4A

Eff. 09-11-1990 Rev. 09-01-2006

When Class 4A Seeding Mixture is used, delete Prairie Dropseed as called for in Table 1 under Article 250.07 of the Standard Specifications.