Regional Engineers

Maureen M. Addis

Special Provision for Portland Cement Concrete Sidewalk

April 21, 2017

This special provision was developed by the Bureau of Design and Environment to clarify the method of measurement for the side curbs and side flares of sidewalk curb ramps.

This special provision should be inserted into contracts containing portland cement concrete sidewalk.

The districts should include the BDE Check Sheet marked with the applicable special provisions for the August 4, 2017 and subsequent lettings. The Project Coordination and Implementation Section will include a copy in the contract.

This special provision will be available on the transfer directory April 21, 2017.

80385m

# portland Cement Concrete sidewalk (BDE)

Effective: August 1, 2017

Revise the first paragraph of Article 424.12 of the Standard Specifications to read:

“**424.12 Method of Measurement.** This work will be measured for payment in place and the area computed in square feet (square meters). Curb ramps, including side curbs and side flares, will be measured for payment as sidewalk. No deduction will be made for detectable warnings located within the ramp.”

80385